Line marking for **REGUPOL** running tracks, multi-use games surfaces and re-topping systems

**Proof of delivery**

**REGUPOL BSW GmbH**

Am Hilgenacker 24

57319 Bad Berleburg (Germany)

+49 2751 803-0

info@regupol.de

[www.regupol.com](http://www.regupol.com)

| **Item** | **Quantity** | **Scope of performance** | **Unit price** | **Total**  |
| --- | --- | --- | --- | --- |
| 1 |  | Supply, survey and professionally apply track line marking in compliance with DLV and/or World Athletics guidelines for a competition/training type track with … oval lanes and … lanes in the sprint section,in UV-resistant 2-component PUR paint, colour coordinated with the installed synthetic surface.Optional: Start lines for 80 m, 75 m and 50 m sprints, hurdle positions and lane numbers in the start and finish areas are also to be applied. | flat rate | € |
| 2 |  | Running track surveying in compliance with DLV and / or World Athletics guidelines for a competition / training type track… with oval lanes and … lanes in the sprint section, by a qualified surveyor, who shall also issue a track certificate (in triplicate), and prepare a coloured line marking plan for the facility. | flat rate | € |
| 3 |  | Provision of riveted or bolted running track event markers made from coloured weather-proof aluminium sheets in compliance with DLV / World Athletics guidelines for a competition / training type track with … oval lanes and … lanes in the sprint section. | flat rate | € |
| 4 | lfm. | Supply, survey and professionally apply runway markings / throwing arcs for:long jump / triple jump / pole vault / javelin, 5 cm or 7 cm in width,in UV-resistant 2-component PUR paint, colour coordinated with the installed synthetic surface. |  | € |

| **Item** | **Quantity** | **Scope of performance** | **Unit price** | **Total**  |
| --- | --- | --- | --- | --- |
| 5 |  | Supply, survey and professionally apply marking lines and dots with UV-resistant 2-component PUR paint, colour coordinated with the installed synthetic surface. | flat rate | € |
| 6 | lfm. | Supply, survey and professionally apply marking lines, marks and dots for the following venues: …………………………………………………………………….in compliance with the guidelines of the relevant sports associations in UV-resistant 2-component PUR paint, colour coordinated with the installed synthetic surface. | flat rate | € |

**Total amount: €**